**Angled stainless steel grab bar 135°, bright, 400 x 400mm**

UltraPolish bright polished stainless steel, 2 fixing points

Ø 32mm

Reference: **5081P2**

Specification description

Angled grab bar 135° for people with reduced mobility, Ø 32mm.

For use as a handrail (horizontal part) or as a grab bar (135° part) for WCs, showers or baths.

 Universal for either left or right side.

Dimensions: 400 x 400mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, non-porous uniform surface for easy maintenance and hygiene.

Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 3-hole, 304 stainless steel plate, Ø 72mm.

Fixing plates and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty.

CE marked.