**Upright shower bar with sliding shower head holder**

UltraSatin polished satin stainless steel

Ø 32mm

Reference: **5460S**

Specification description

Upright shower riser rail with shower head holder Ø 32mm for people with reduced mobility.

Can be used as a vertical grab bar and a shower head rail for showers or baths.

Chrome-plated metal shower head holder with ergonomic locking ring.

Possible to add a sliding soap dish (order separately).

Height: 1,150 mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraSatin polished satin finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured to wall by a 3-hole plate, 304 stainless steel, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty. CE marked.