**Riser rail with shower head holder in anti-bacterial white Nylon**

Bright white NylonClean anti-bacterial HR Nylon

Ø 32mm

Reference: **5460N**

Specification description

Upright shower raiser rail Ø 32mm with shower head holder for people with reduced mobility.

Can be used as a vertical grab bar and a shower head rail.

Nylon HR shower head holder with ergonomic locking ring. Possible to add a soap dish holder (order separately).

NylonClean anti-bacterial Nylon: optimal protection against bacterial development.

Suitable for intensive use in public places or the healthcare sector.

High-strength polyamide (Nylon) and polymer: with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 6-hole plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Height: 1,150mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty. CE marked.