**U-shaped toilet roll holder with spindle**

For toilet rolls

White powder-coated 304 stainless steel

Reference: **4081EW**

Specification description

Wall-mounted U-shaped toilet roll holder.

Toilet roll holder

Bacteriostatic white powder-coated 304 stainless steel.

Tube Ø 20mm, 1mm thick.

Concealed fixings.

30-year warranty.