**TEMPOMIX 2 time flow mixer**

(AB) Anti-blocking model, stopcocks

Standard temperature control

Reference: **700001**

Specification description

Deck-mounted time flow basin mixer:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Tamperproof, scale-resistant flow straightener.

Chrome-plated brass body.

PEX flexibles with stopcocks F3/8", filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Side temperature control with standard lever and adjustable maximum temperature limiter.

AB anti-blocking system: water only flows when push-button is released.

30-year warranty.