**TEMPOMIX time flow shower panel**

Time flow single control

Top inlet, fixed head, alu

Reference: **790300**

Specification description

Time flow shower panel with fixed shower head:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via stopcocks M½".

TEMPOMIX shower mixer with adjustable maximum temperature limiter.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filters and non-return valves.

Shower panel suitable for people with reduced mobility.

30-year warranty.