**TEMPOMATIC electronic shower valve**

Electronic

Cross wall for 150mm walls

Reference: **452150**

Specification description

Cross wall electronic shower valve:

TEMPOMATIC electronic valve for mixed water supply.

For walls ≤ 155mm.

Power supply by electronic unit with solenoid valve ½".

230/12V transformer.

2 operation modes:

- Automatic activation using presence detection.

- Voluntary ON/OFF activation by passing the hand in front of sensor ~10 cm.

Duty flush (~60 seconds every 24 hours after the last use).

Adjustable time flow from 30 to 60 seconds.

Flow rate 20 lpm.

Chrome-plated solid brass.

Wall plate flush to the wall.

Threaded rods can be cut-to-size.

Electronic shower valve suitable for people with reduced mobility.

30-year warranty.