**PREMIX NANO thermostatic mixing valve**

For mixed water from 34 - 60°C

Chromed body, HW inlet F3/8" CW and outlet M3/8"

Reference: **732216**

Specification description

Thermostatic mixing valve for mixed water distribution from 34 - 60°C:

For 1 to 2 taps or 1 shower.

Anti-scalding safety: automatic water shut-off in case of hot or cold water supply failure.

Temperature pre-set at 38°C, can be adjusted by the installer from 34 - 60°C.

Non-return valves and filters.

Minimum flow rate for operation: 3 lpm.

Thermal shocks are possible.

Polished chrome body, hot water inlet F3/8", cold water inlet M3/8"and mixed water outlet M3/8".

30-year warranty.