**TEMPOSTOP time flow urinal valve**

Time flow 7 seconds

Straight ¾"

Reference: **779000**

Specification description

Exposed time flow urinal valve:

For siphon action urinals.

For wall-mounted installation.

Time flow ~7 seconds.

Flow rate pre-set at 0.25 l/sec. at 3 bar, can be adjusted.

Compatible with rain water.

Chrome-plated solid brass body M¾".

Straight for in-line inlet.

30-year warranty.