**Flush tube**

For WC pans with TEMPOMATIC, TEMPOFLUX or TEMPOCHASSE

PVC

Reference: **769400**

Specification description

Cross wall/recessed flush tube for WC pans:

For TEMPOMATIC, TEMPOFLUX 1, TEMPOFLUX 2, TEMPOFLUX 3 and TEMPOCHASSE.

PVC tube for recessed or cross wall installation.

Ø 26/32mm (without connection washer).

L. 434mm, H. 780mm.

30-year warranty.