**TEMPOMATIC PRO electronic tap**

Mains supply, Ø 15mm conical inlet

Swivelling removable spout, smooth interior

Reference: **44525315**

Specification description

Deck-mounted electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 4 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Shock-resistant infrared presence detection sensor.

Chrome-plated solid brass body with fixing reinforced by 2 stainless steel rods.

PEX flexible with filter and solenoid valve Ø 15mm for compression fittings.

360° swivelling spout with smooth interior (reduces bacterial development).

Removable spout for cleaning.

Anti-blocking security.

Two shut-off options:

Standard mode: timed flow with automatic shut-off.

ON/OFF mode: user shuts off voluntarily or automatic shut-off after 30 minutes of flow.

Thermal shocks are possible.

30-year warranty.