**TEMPOMATIC Electronic tap**

Mains supply, conical inlet Ø 15mm

165mm cross wall

Reference: **44115715**

Specification description

Cross wall electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Shockproof infrared presence detection sensor for wall ≤ 165mm.

Anti-blocking security.

Solenoid valve with filter and Ø 15mm conical inlet.

Chrome-plated fixed spout L. 170mm for wall ≤ 165mm with anti-rotating pin.

Threaded rods can be cut to size.

30-year warranty.