**Wall-mounted BOB washbasin**

Polished satin 304 stainless steel - with concealed trap

Without tap hole

Reference: **120130**

Specification description

Wall-mounted washbasin.

Basin internal diameter: 310mm.

Clean and simple design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed trap.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

With no tap hole.

Supplied with 1½" waste and trap.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 5.5kg.

30-year warranty.

[Formerly ref: 3411130000]