**Wall-mounted SD drinking fountain**

Polished satin 304 stainless steel

With built-in tap

Reference: **180800**

Specification description

Wall-mounted drinking fountain.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Supplied with bubbler tap: chrome-plated, instant shut-offand adjustable flow rate, inlet M⅜".

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Waste outlet 1¼" trap.

Supplied with fixing elements. Weight: 2.4kg.

30-year warranty.

[Formerly ref: 0811080000]