**Twin toilet roll holder**

For toilet rolls

White powder-coated 304 stainless steel

Reference: **510082W**

Specification description

Wall-mounted toilet roll holder.

Twin toilet roll holder.

Tube Ø 20mm, 1mm thick.

Bacteriostatic white powder-coated 304 stainless steel.

Concealed fixings.

30-year warranty.