**Countertop ALGUI washbasin**

Dual finish 304 stainless steel - Countertop

Reference: **120112**

Specification description

Countertop washbasin, Ø 375mm.

Suitable for use with wall-mounted or extended mixer/tap.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Dual finish: bright polished basin interior and polished satin exterior.

One-piece, seam-free pressed bowl.

Rounded edges prevent injury.

Supplied with 1¼" waste.

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 3.8kg.

30-year warranty.