**DELTA wall-hung urinal**

Dual finish 304 stainless steel - Rear water inlet

Reference: **134772**

Specification description

Wall-hung individual rimless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel.

Dual finish: bright polished pan interior and polished satin exterior.

Stainless steel thickness: 1.2mm.

Rear (recessed) water inlet.

Recessed waste outlet. Concealed trap.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with 1½" P trap. Supplied with fixing elements and theft prevention TORX security screws.

CE marked. Complies with European standard EN 13407 for 2L flush.

Weight: 7.5kg.

30-year warranty.