**SECURITHERM shower panel**

Dual control thermostatic mixer

Top inlet, fixed shower head and hand set

Reference: **792340**

Specification description

Dual control thermostatic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlets via in-line stopcocks M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C; with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Soft-touch operation.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

Handset with removable flexible via rapid push-fit STOP connector.

~30 second time flow valve with soft-touch operation to control fixed ROUND shower head.

Non-time flow 1/4-turn valve to control handset on flexible hose (wall support supplied).

Concealed fixings.

Filters and non-return valves.

Shower panel suitable for people with reduced mobility.

30-year warranty.