**FINO WF waterless urinal**

Polished satin 304 stainless steel

Reference: **135010**

Specification description

Wall-hung individual waterless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.2mm.

Recessed horizontal waste outlet.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

1½" waste outlet.

Supplied with a silicone membrane to prevent bad smells.

Supplied with fixing elements.

Weight: 3.5kg.