**Divider for wall-hung trough urinal**

Polished satin 304 stainless steel - H. 430mm

Reference: **100900**

Specification description

Divider for wall-hung trough urinals.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Install directly onto the urinal in the desired position.

Only suitable for wall-hung trough urinals refs 130100, 130110 and 130120.