**TEMPOFIX 3 frame system for urinals**

For FINO and DELTACÉRAM urinals

Reference: **543130**

Specification description

Frame system for FINO and DELTACÉRAM urinals:

Black powder-coated steel frame for wall-mounted installation.

Fixes to floor and load-bearing walls, anchoring bolts supplied.

Adjustable bracket.

Frame height can be adjusted from 0 - 200mm.

Ø 50mm soil pipe with waterproof seal.

Delivered pre-mounted.

Compatible with solid wall finishes from 13 - 110mm.

Compatible with HYBRIMATIC urinals (FINO or DELTACÉRAM).

Can also be used with any urinal on the market with flexible supply.

30-year warranty.