**TEMPOMATIC MIX 5 electronic basin mixer**

Battery-operated

Standard lever, without stopcocks

Reference: **499106**

Specification description

Deck-mounted electronic basin mixer:

Operated by CR123 Lithium 6V batteries.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated metal body.

PEX flexibles F3/8" with filters and non-return valves.

Fixing reinforced by two stainless steel rods.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.