**TEMPOFIX 3 self-supporting frame system for WCs**

For time flow or battery-operated electronic valves - Ø 100mm

Self-supporting, for walls from 10 to 120mm

Reference: **564065**

Specification description

Self-supporting frame system for wall-hung WCs, kit 1/2:

Black powder-coated steel frame:

- With large feet for fixing to load-bearing floors.

- Frame height can be adjusted from 0 - 200mm (with 1m mark).

- Compatible with solid walls from 10 - 120mm.

- Ø 32mm flush tube with Ø 55mm connection washer.

- PVC soil pipe, Ø 100mm outlet to glue to waterproof seal, with 2 setting positions.

Recessed waterproof housing: for flush system without cistern, directly connected to pipework.

- Compatible with electronic or time flow WC valve.

- Compatible with CR123 6V Lithium batteries.

- Backflow prevention device inside the housing.

- Integrated stopcock and flow rate regulation.

Supplied pre-mounted.

30-year warranty.

Order with control plate references 464006, 464056, 465006, 465056, 763000, 763040 or 763041or 763030.