**Wall-mounted TEMPOFIX 3 frame system for WCs**

For TEMPOFLUX 2 time flow valve - Outlet Ø 100mm

Wall-mounted, for walls from 10 to 35mm

Reference: **578300**

Specification description

Wall-mounted frame system for wall-hung WCs, kit 1/2:

Black powder-coated steel frame:

- Fixes to load-bearing walls.

- Frame height can be adjusted from 0 - 200mm (with 1m mark).

- For wall finishes from 10 to 35mm.

- Ø 32mm flush tube with Ø 55mm connection washer.

- Ø 100mm soil pipe and PVC collar with waterproof seal, with 2 settings positions.

Fitted with a TEMPOFLUX 2 time flow direct flush:

- Flush system without cistern: directly connected to pipework.

- Vacuum breaker.

- Integrated stopcock and flow rate/volume adjuster.

- Solid brass body and shock-resistant, scale-resistant mechanism.

- In-line inlet M¾".

- Compatible with rain water.

Delivered pre-mounted.

30-year warranty.

Order with control plate references 578222, 578212 or 578230.