**Countertop QUADRA washbasin**

Matte black 304 stainless steel - Countertop

Reference: **120650BK**

Specification description

Countertop, semi-recessed washbasin, 380x380mm.

Suitable for use with wall-mounted or extended mixer/tap.

Basin internal diameter: 310mm.

Cutout diameter: 310mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Matte black Teflon® finish.

One-piece, seam-free pressed bowl.

Rounded edges prevent injury.

Supplied without waste. Waste with black finish can be added (6110BK) or chrome finish (6110).

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 3kg.

30-year warranty.