**BIOFIL 2 month spout filter**

Sterile

Reference: **20040**

Specification description

Single use removable BIOFIL anti-Legionella and all-germ spout.

Can be installed instead of removable BIOCLIP spouts (no need for any tools or to shut off the water supply).

Membrane type: tubular microfiltration.

Membrane material: Polyethylene.

pore cut-off threshold: 0.1µm nominal-rated, sterilising grade.

Filtration surface area 1,200 cm².

Filtration flow rate: 6 lpm at 3 bar (filter only, excludes any flow rate restriction in the mixer/tap).

Maximum upstream pressure at the point-of-use: 5 bar.

Maximum lifespan: 2 months after installation.

Compatible with and resistant to thermal and chemical shocks.

Sterile filter.

Weight: 40g.

Reference for a single unit. Must be ordered in multiples of 10.

Packaged in boxes of 10 units.