**Brass BIOCLIP spout**

Spout L.70mm Ø 28mm for mixers with removable spouts

2 per pack

Reference: **20004**

Specification description

Removable brass BIOCLIP spout L. 70mm Ø 28mm or easy cleaning/descaling of the interior or autoclaving.

Spouts fitted with a hygienic flow straightener, suitable for fitting a point-of-use BIOFIL filter.

Spout with smooth interior reduces bacterial development.

The second spout enables continuous use during cleaning/descaling of the first spout.

Suitable for all mixers and taps with BIOCLIP spout.

2 per pack.