DELABIE_C100M3550506S

**Straight grab bar Ø 32mm, 600mm**

Reference: 50506S

Specification Description

Straight grab bar for people with reduced mobility.

Tube Ø 32mm, 600mm centres, 1.5mm thick.

For use as a handrail and grab or support bar for WCs, showers or baths.

Bacteriostatic 304 stainless steel tube.

UltraSatin polished satin stainless steel, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixing, secured to wall by a 3-hole, 304 stainless steel plate, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.