**Angled Nylon grab bar 135°, white, anti-bacterial, 400 x 400mm**

Bright white HR anti-bacterial Nylon, NylonClean, 3 fixing points

Ø 32mm

Reference: **5081N**

Specification description

Angled grab bar 135°, Ø 32mm, for people with reduced mobility.

Angled grab bar made from bright white HR Nylon.

For use as a handrail (horizontal part) or as a grab bar (135° part) for WCs, showers or baths.

NylonClean anti-bacterial treatment: optimal protection against bacterial and mould development.

Universal for either left or right side.

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning.

Anti-UV treatment: prevents yellowing.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

3 fixing points prevent the hand from getting trapped wrist and simplify installation.

Concealed fixings, secured to wall by a 6-hole plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Dimensions: 400 x 400mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty.

CE marked.