**Mechanical basin mixer**

Wall-mounted mixer with swivelling spout L. 150mm, sculptured lever

With STOP/CHECK connectors

Reference: **2446**

Specification description

Wall-mounted mechanical basin mixer.

 Flat, swivelling under spout L. 150mm with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Body and spout with smooth interiors and low water volume (reduces bacterial development).

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter .

Body and spout with smooth interiors and low water volume (reduces bacterial development).Flow rate reguated at 5 lpm.

Chrome-plated brass body.

Sculptured control lever.

Supplied with STOP/CHECK connectors M1/2" M3/4" ideal for hospitals.

30-year warranty.