**Straight stainless steel grab bar, bright, Ø 25mm, 300mm**

UltraPolish bright polished stainless steel

Ø 25mm

Reference: **5055P2**

Specification description

Straight grab bar for people with reduced mobility.

Tube Ø 25mm, 300mm centres, 1.2mm thick.

For use as a handrail and grab or support bar for WCs, showers or baths.

Grab bar for toilets made from bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured to wall by a 3-hole plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 115kg.

30-year warranty.

CE marked.