**Straight stainless steel grab bar, satin, Ø 32mm, 400mm**

UltraSatin polished satin stainless steel

Ø 32mm

Reference: **50504S**

Specification description

Straight grab bar for people with reduced mobility.

Tube Ø 32mm, 400mm centres.

For use as a handrail and grab or support bar for WCs, showers or baths.

Straight grab bar made from bacteriostatic 304 stainless steel.

UltraSatin polished satin stainless steel, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates made from 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 250kg. Maximum recommended user weight: 170kg.

30-year warranty.

CE marked.