**L-shaped stainless steel shower grab bar, bright, H. 1,150mm**

UltraPolish bright polished stainless steel, left model

Ø 32mm

Reference: **5071GP2**

Specification description

L-shaped grab bar Ø 32mm, for PRM, left model.

Helps the user stand and secures movement in the bath or shower.

Can be used as a shower rail by adding a shower head holder and/or soap dish.

Dimensions: 1,150 x 450mm.

Tube thickness: 1.5mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

Bar comes with 30-year warranty. CE marked.