**Right angled, shower grab bar (right model) with vertical bar, Ø 32mm**

UltraPolish bright polished stainless steel, right model

Ø 32mm

Reference: **5100DP2**

Specification description

Angled, two-wall grab bar with vertical bar for PRM, Ø 32mm. Right model.

Can be used as a support bar and to support the user in an upright position.

Helps and secures entry and movement in the shower.

Can be used as a shower rail by adding a sliding shower head holder and/or soap dish.

Dimensions: 1,265 x 560 x 660mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty. CE marked.