**Angled shower grab bar with vertical bar, bright stainless steel**

UltraPolish bright polished stainless steel, right model

Ø 32mm, for hung shower seats

Reference: **5481DP2**

Specification description

Angled, two-wall shower grab bar with vertical bar Ø 32mm, for people with reduced mobility.

Right model.

Can support a removable shower seat (order separately).

Can be used as a support bar and to support the user in an upright position.

Helps and secures entry and movement in the shower.

Can be used as a shower rail by adding a shower head holder and/or soap dish.

Dimensions: 1,150 x 750 x 750mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 3-hole cover plate, Ø 72mm.

304 stainless steel plates and covers.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty. CE marked.