**Basic T-shaped white grab bar**

White powder-coated stainless steel

Ø 32mm

Reference: **35440W**

Specification description

T-shaped shower grab bar with sliding vertical bar for people with reduced mobility.

White powder-coated stainless steel tube.

Upright position can be adjusted during installation: can be moved to the left or the right.

Dimensions: 1,150 x 500mm, Ø 32mm.

Concealed fixings, secured to wall by a 3-hole stainless steel plate.

CE marked.

30-year warranty.