**Comfort backrest for WCs**

Bright white HR Nylon structure

Black polyurethane

Reference: **510629N**

Specification description

Comfort backrest for WCs, for people with reduce mobility.

Structure made from white, high strength polyamide (Nylon).

Backrest for toilets made from soft polyurethane.

Tube Ø 32mm.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Dimensions: 150 x 575 x 173mm.

30-year warranty. CE marked.