**Backrest for Comfort shower seat**

Backrest for shower seats

UltraPolish bright stainless steel structure

Reference: **510429**

Specification description

HR Comfort backrest.

Backrest for shower seats for disabled people or for people with reduced mobility.

Large model for shower seats ref. 510420 and 510430.

Anti-bacterial treatment on the backrest: optimal protection against bacterial development and mould.

Suitable for intensive use in public places or the healthcare sector.

Removable solid backrest made from high strength polymer.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products (Betadine®) and cleaning.

Anti-UV treatment.

Warm to the touch.

Bacteriostatic 304 stainless steel structure Ø 32mm.

UltraPolish bright polished finish.

Supplied with stainless steel screws for concrete walls.

Dimensions: 56 x 420 x 410mm.

Backrest for shower seats with 30-year warranty. CE marked.