**Wall-mounted toilet brush set**

Model with anti-theft lock for fixing

Polished satin 304 stainless steel

Reference: **4048S**

Specification description

Wall-mounted toilet brush set.

Wall-mounted robust model with toilet brush and anti-theft lock for fixing.

Bacteriostatic polished satin 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used.

Stainless steel body 1mm thick.

Dimensions: Ø 90mm x 330mm.

30-year warranty.