**Hand dryer automatically activated by optical cell, with 360° nozzle**

Optical cell

White enamelled steel

Reference: **6615**

Specification description

Automatic hand dryer.

Vandal-resistant model.

Automatically activated via optical cell.

360° rotating nozzle.

Metal thickness: 1.2mm.

White, enamelled cast steel cover.

Dimensions: 210 x 280 x 220mm.

Weight: 3.5kg.

Power: 2,000W.50-60 Hz.

Air flow: 95 l/sec.

Low noise level: 68 dBA.

Class II maximum security (double insulated electrical appliance), IP23.

CE, TÜV GS.

Warranty: 3 years.