**Towel rail**

Ø 20mm, 2 rails

Bright polished stainless steel

Reference: **510790P**

Specification description

Towel rail for bathrooms.

Twin rail designer towel rail.

Robust model.

Ø 20mm and Ø 16mm rails, length 600mm.

Bright polished 304 bacteriostatic stainless steel.

Towel rail with concealed fixings.

30-year warranty.