**SECURITHERM BIOCLIP thermostatic sink mixer**

Wall-mounted thermostatic sequential mixer

Standard connectors, removable disposable spout

Reference: **H9610S**

Specification description

Wall-mounted SECURITHERM thermostatic sink mixer.

Thermostatic sequential mixer: opens and closes with cold water.

No risk of cross flow between hot and cold water.

No non-return valves on the inlets.

Wall-mounted mixer supplied with 1 removable, disposable spout made from recyclable Hostaform® L. 125mm.

Anti-scalding failsafe: shuts off automatically if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant thermostatic sequential cartridge for sequential control of flow rate and temperature.

Temperature can be adjusted from cold water up to 40°C with maximum temperature limiter set at 40°C.

Thermal and chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 7 lpm.

Chrome-plated brass body.

No manual contact thanks to Hygiene control lever L. 146mm.

Mixer with 150mm centres supplied with offset standard connectors M1/2" M3/4".

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Sequential mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.