**Mechanical mixer for sinks or troughs**

Single hole mechanical mixer with swivelling spout H. 155mm L. 230mm

Mixer with Hygiene control lever

Reference: **2510L**

Specification description

Deck-mounted mechanical sink mixer.

Single hole mechanical mixer with swivelling spout H. 155mm L. 230mm fitted with hygienic flow straightener.

Spout suitable for fitting a BIOFIL point-of-use filter.

Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors.

Body and spout made from chrome-plated brass.

Hygiene control lever L. 200mm.

Flow rate set at 9 lpm at 3 bar.

Supplied with PEX flexibles F3/8".

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.