**Stainless steel BIOCLIP spout**

Spout L. 129mm Ø28mm for mixers with removable spouts

2 per pack

Reference: **20002**

Specification description

Removable stainless steel BIOCLIP spout L. 129mm Ø 28mm for cleaning and internal disinfection or autoclaving.

Spouts fitted with a hygienic flow straightener, suitable for fitting a BIOFIL point-of-use filter.

Spout with smooth interior reduces bacterial development.

The second spout enables continuous use during the cleaning/descaling of the first spout.

Suitable for all mixers/taps with a BIOCLIP spout.

Supplied in packs of 2.