**Mechanical mixer for basins**

Single hole, single control tall mixer with ceramic cartridge

Mechanical mixer with fixed spout H.165 L.140

Reference: **2565T1**

Specification description

Deck-mounted mechanical basin mixer.

Single hole, single control mixer with fixed spout H. 165mm L. 140mm.

Tall mixer with BIOSAFE hygienic outlet suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduces bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water supply.

Flow rate regulated at 5 lpm.

Chrome-plated brass body and base.

Hygiene control lever L. 185mm requires no manual contact.

F3/8" PEX flexibles.

Reinforced fixings via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.