**Mechanical mixer for sinks or troughs**

Single hole, single control tall mixer with ceramic cartridge

Mechanical mixer with swivelling spout H.305 L.140

Reference: **2565T3**

Specification description

Deck-mounted tall mechanical sink mixer.

Single hole, single control mixer with fixed spout H. 305mm L. 140mm.

Tall mixer with hygienic flow straightener suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Thermal shocks are easy to undertake without removing control lever or shutting off the cold water.

Flow rate limited to 9 lpm at 3 bar.

Chrome-plated brass body and base.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8".

Reinforced fixings by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement or care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.