**Mechanical basin mixer**

Wall-mounted mixer with swivelling spout L. 150, Hygiene lever L. 150

With offset STOP/CHECK connectors

Reference: **2446L**

Specification description

Wall-mounted mechanical basin mixer.

Swivelling, flat under-spout L. 150mm in chrome-plated brass with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Ø 40mm ceramic cartridge and pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduce niches where bacteria can develop).

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Hygiene control lever L. 150mm.

Supplied with STOP/CHECK connectors, M1/2" M3/4", ideal for hospitals.

30-year warranty.