**Mechanical shower mixer**

Wall-mounted single control mixer, sculptured lever

With offset STOP/CHECK connectors

Reference: **2539**

Specification description

Wall-mounted single control mechanical shower mixer.

Ø 40mm classic ceramic cartridge and pre-set maximum temperature limiter.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset STOP/CHECK wall connectors M1/2" M3/4".

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Shower mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.