**Shower riser rail with mechanical mixer**

Shower kit with Securitouch mixer with smooth interior

With offset STOP/CHECK connectors

Reference: **2739KIT**

Specification description

Shower riser rail with single control mechanical mixer.

Wall-mounted shower kit with shower mixer.

• Wall-mounted single control mixer with Securitouch thermal insulation to prevent burns.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset STOP/CHECK wall connectors, M1/2" M3/4".

• Sliding shower head holder (ref. 813) on a chrome-plated riser rail (ref. 821) with soap dish and flexible shower hose (ref. 836T1).

• Shower head retaining collar (ref. 830).

Shower riser rail is ideal for healthcare facilities, retirement homes, hospitals and clinics.

Mechanical mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.