**Siphon**

With horizontal outlet

Chrome-plated brass

Reference: **517000**

Specification description

Trap for urinals or basins with horizontal outlet:

Inlet F1¼".

Horizontal outlet Ø 32mm with nut.

Water level 50mm.

Chrome-plated brass.

30-year warranty.